ASSIGNMENT – 4

Ultrasonic sensor simulation in Wokwi

|  |  |
| --- | --- |
| Assignment Date | 25 October 2022 |
| Student Name | Jothika.S |
| Student Roll Number | 713519CEEC503 |
| Maximum Marks | 2 Marks |
| Team ID | PNT2022TMID07793 |
| Project Name | Real-Time River Water Quality Monitoring and Control System. |

**QUESTIONS:**

Write code and connections in wokwi for the ultrasonic sensor. Whenever the distance is less than 100 CMS send an "alert" to the IBM cloud and display in the device recent events

**CODE:**

#include <WiFi.h>

#include <PubSubClient.h>

WiFiClient wifiClient;

String data3;

#define ORG "3yngbh"

#define DEVICE\_TYPE "Assignment"

#define DEVICE\_ID "1234"

#define TOKEN "234567890"

#define speed 0.034 #define led 14

char server[] = ORG ".messaging.internetofthings.ibmcloud.com"; char publishTopic[] = "iot-2/evt/shreedharen/fmt/json"; char topic[] = "iot-2/cmd/led/fmt/String"; char authMethod[] = "use-token-auth";

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

PubSubClient client(server, 1883, wifiClient);

const int trigpin=5; const int echopin=18;

String command;

String data="";

long duration;

float dist;

void setup()

{

Serial.begin(115200); pinMode(led, OUTPUT); pinMode(trigpin, OUTPUT); pinMode(echopin, INPUT);

wifiConnect(); mqttConnect();

}

void loop() { bool isNearby = dist < 100; digitalWrite(led, isNearby);

publishData();

delay(500);

if (!client.loop()) {

mqttConnect();

}

}

void wifiConnect() {

Serial.print("Connecting to "); Serial.print("Wifi"); WiFi.begin("Wokwi-GUEST", "", 6);

while (WiFi.status() != WL\_CONNECTED) { delay(500); Serial.print(".");

}

Serial.print("WiFi connected, IP address: "); Serial.println(WiFi.localIP()); }

void mqttConnect() { if (!client.connected()) {

Serial.print("Reconnecting MQTT client to "); Serial.println(server); while (!client.connect(clientId, authMethod, token)) {

Serial.print(".");

delay(500);

}

initManagedDevice();

Serial.println();

}

}

void initManagedDevice() { if (client.subscribe(topic)) {

// Serial.println(client.subscribe(topic));

Serial.println("IBM subscribe to cmd OK");

} else {

Serial.println("subscribe to cmd FAILED");

} }

void publishData()

{ digitalWrite(trigpin,LOW); digitalWrite(trigpin,HIGH); delayMicroseconds(10); digitalWrite(trigpin,LOW); duration=pulseIn(echopin,HIGH); dist=duration\*speed/2; if(dist<100){

String payload = "{\"Alert Distance\":"; payload += dist;

payload += "}";

Serial.print("\n");

Serial.print("Sending payload: "); Serial.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

Serial.println("Publish OK");

}

}

if(dist>100){

String payload = "{\"Distance\":"; payload += dist; payload += "}";

Serial.print("\n");

Serial.print("Sending payload: "); Serial.println(payload);

if(client.publish(publishTopic, (char\*) payload.c\_str())) {

Serial.println("Publish OK");

}else {


Serial.println("Publish FAILED");

}


}

}

**.json CODE:**




**CIRCUIT DIAGRAM:**



**Wokwi simulation link:**

https://wokwi.com/projects/347107114793042514

**WOKWI OUTPUT:**



**IBM CLOUD OUTPUT:**

