SPRINT-4

|  |  |
| --- | --- |
| **TEAM ID** | PNT2022TMID07793 |
| **PROJECT TITLE** | REAL-TIME RIVER WATER QUALITY MONITORING AND CONTROL SYSTEM |
| **DATE** | 13 NOVEMBER 2022 |
| **MAXIMUM MARK** |  |

# CODE FOR ARDUINO:

#include <OneWire.h>

#include <DallasTemperature.h> #define ONE\_WIRE\_BUS 5

OneWire oneWire(ONE\_WIRE\_BUS); DallasTemperature sensors(&oneWire); float Celcius=0; float Fahrenheit=0; float voltage=0; const int analogInPin = A0; int sensorValue = 0; unsigned long int avgValue; float b; int buf[10],temp; void setup(void)

{

Serial.begin(9600); sensors.begin(); int sensorValue = analogRead(A1); voltage = sensorValue \* (5.0 /

1024.0);

} void loop(void) { sensors.requestTemperatures(); Celcius=sensors.getTempCByIndex(0); Fahrenheit=sensors.toFahrenheit(Celcius); for(int i=0;i<10;i++) { buf[i]=analogRead(analogInPin); delay(10); } for(int i=0;i<9;i++) { for(int j=i+1;j<10;j++)

}

} } for(int i=2;i<8;i++) avgValue+=buf[i]; float pHVol=(float)avgValue\*5.0/1024/6; float phValue = -5.70 \* pHVol + 21.34;

Serial.println(phValue); Serial.print("pH");

Serial.print(" C "); Serial.print(Celcius);

Serial.print(voltage); Serial.print("V"); delay(10000);

}

# CODE IMPLEMENTATION:

import serial import time import csv import numpy as np import matplotlib.pyplot as plt ser = serial.Serial('/COM6',9600) ser\_bytes = ser.readline(10) print (ser\_bytes) ser.flushInput() while True:

try:

ser\_bytes = ser.readline() decoded\_bytes = float(ser\_bytes[0:len(ser\_bytes)-2].decode("utf-8")) print(decoded\_bytes)

temp = float(decoded\_bytes(1:3)) turb = float(decoded\_bytes(4:6)) pH = float(decoded\_bytes(6:8)) with open("test\_data.csv","a") as f: writer = csv.writer(f,delimiter=",") writer.writerow([time.time(),decoded\_bytes]) except: print("Keyboard Interrupt") ser.close() break() t = np.arange(0.0, 2.0, 0.01) s = 1 + np.sin(2\*np.pi\*t) plt.plot(t, s) plt.xlabel('time (s)') plt.ylabel('Celsisus (C)')

Serial.begin(9600); sensors.begin(); int sensorValue = analogRead(A1); voltage = sensorValue \* (5.0 / 1024.0);

}

void loop(void)

{

sensors.requestTemperatures();

Celcius=sensors.getTempCByIndex(0); Fahrenheit=sensors.toFahrenheit(Celcius); for(int i=0;i<10;i++)

{

buf[i]=analogRead(analogInPin); delay(10);

}

for(int i=0;i<9;i++)

{

for(int j=i+1;j<10;j++)

{

if(buf[i]>buf[j])

{

temp=buf[i]; buf[i]=buf[j]; buf[j]=temp;

}

n = 256

X = np.linspace(-np.pi, np.pi, 256, endpoint=True) C,S = np.cos(X), np.sin(X) plt.plot(X, C) plt.plot(X,S) plt.show()

print ("Visualization of real time sensor Data.") print("/n") while True:

try:

ser\_bytes = ser.readline() decoded\_bytes = float(ser\_bytes[0:len(ser\_bytes)-2].decode("utf-8")) print(decoded\_bytes) temp = float(decoded\_bytes(1:3)) turb = float(decoded\_bytes(4:6)) pH = float(decoded\_bytes(6:8)) with open("test\_data.csv","a") as f: writer = csv.writer(f,delimiter=",")

np.arange(0.0, 2.0, 0.01) s = 1 + np.sin(2\*np.pi\*t) plt.plot(t, s)

# ARDUINO OUTPUT:

